**ULXDBT - Universal Open Water Dual Beam Ducer w/Temp - 857224002415 - COPY-SPEC**

**Copy**

This transducer works best with MarCum M5, LX-5, LX-6, LX-7, LX-9, and MX-7gps Dual Beam Systems. Also compatible with VX-1i, LX-1, LX-2, LX-3, LX-3TC, LX-3TCi, and M3 Single Beam Systems, with the transducer defaulting to the 20-degree cone. Equipped with temp sensor for use with all 2012-13 (and newer) LX Digital Series Systems. Transom or trolling motor mounted capability.

**Features/Specs**

* Dual Beam (8 and 20 Degree) Transducer with Temp Sensor
* 20 Foot Cable
* Dual Beam Transducer Can Be Mounted to the Transom or Trolling Motor with One Universal Bracket System
* Includes All Transom Mounting Hardware and Power Cord

**Weight and Dimensions**

WEIGHT: 2 Pounds

HEIGHT: 3.5 Inches

WIDTH: 8 Inches

DEPTH: 7 Inches

**Compatible Products**

M5 M5 Flasher System 857224002736

M5L M5L LiFePO4 850013782024

M5LI M5LI Combo 857224002811

LX-7L LX-7L LiFePO4 850013782031

LX-7LI LX-7LI Combo 857224002835

LX-9L LX-9L LiFePO4 850013782055

MX-7gps MX-7gps 850013782048

MX-7gpsLI MX-7gpsLI 857224002989