010-02367-03 GPSMAP® 1243xsv, SideVü, ClearVü and Traditional CHIRP Sonar with Mapping $2,999.99 USD $2,399.99 USD

Product Details

Rebates & Promotions

Images

Videos

Marketing Collateral

Marketing Memos

Overview

Product Specifications

In the Box

Accessories

Physical & Performance

Display Size 10.3" x 6.4"; 12.1" diagonal (26.2 x 16.3 cm; 30.7 cm diagonal)

Power Input 10 to 32 Vdc

Display resolution 1280 x 800 pixels

GPS Yes

Dimension 12.1” x 8.9” x 3.2” (30.8 x 22.8 x 8.2 cm)

Receiver

10 Hz

Waterproof

IPX7

Weight

6.6 lbs (3.0 kg)

Mounting Options Bail, flush or flat (Garmin does not offer any hardware or accessories for a flat-mount installation. Professional tools and knowledge is required.)

Display Type WXGA

Maps & Navigation

Garmin Navionics Vision+™ Yes

Accepts Data Cards

2 microSD cards (back of unit)

Navigation Routes 100

Garmin Navionics+™ Yes

Features

Waypoints

5000

Sailing Features Yes

NMEA 0183 Compatible Yes

Has built-in receiver Yes

USB ports Yes

(Sounder) TOPO Yes

(Sounder) SideVü built-in 260/455/800/1000/1200 kHz

DSC Yes

Touchscreen Yes

LakeVü g3 Ultra Yes

NMEA 2000 Compatible Yes

ActiveCaptain® compatible

yes

Typical current draw at 12 Vdc 1.68 A

NMEA 2000 ports 1

(Sounder) Tide tables Yes

GLONASS Yes

Track points 50,000

Panoptix™ sonar Yes

Connections Garmin Marine Network Ports

2

LakeVü g3 Yes

Supports WAAS Yes

GSD Black Box Sonar Support Yes

Maximum current draw at 12 Vdc 3.56 A

Smart Mode Compatible Yes

Built-in Auto Guidance Yes

Maximum power usage at 10 Vdc 43.0W

BlueChart g3 Yes

Standard Mapping Yes

LakeVu (inland) Yes

Displays sonar Yes

ANT+ (Connectivity) Yes

GCV Black Box Sonar Support Yes

BNC external GPS antenna port No

Connections NMEA0183 Input Ports

1

Spoken audio alerts Yes

BlueChart g3 Vision Yes

Garmin Wi-Fi network (local connection) Yes

J1939 ports 1

Input Touchscreen

Garmin Quickdraw Contours Yes

BLUETOOTH® calling Yes

AIS Yes

Video output ports

1 HDMI

Raster chart support Yes

NMEA 0183 input (Tx) ports 1

OneHelm support Yes

ClearVü built-in 260/455/800/1000/1200 kHz

Tracks 50 saved tracks

Wireless Remote Compatible Yes

Supports Fusion-Link™ compatible radios Yes

Galileo Yes

LiveScope Yes

Power output 1 kW

12-pin transducer ports 1

BlueChart (coastal) Yes

Traditional sonar (dual frequency/beam) built-in (single channel CHIRP, 70/83/200 kHz, L, M, H CHIRP)

GRID (Garmin Remote Input Device) compatible Yes

Video input ports

1 (BNC composite)